Fire Code for Hot Work:

As per National Fire Code Article 5.2.3.1
Section 2

* Fire watch must be maintained at location of hot work for a minimum of one hour following completion of said hot work.
* A final inspection of the hot work location must occur 4 hours after the completion of said hot work.